UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_msg_umq_deregistration_complete_ex_t_stct Struct Reference

Structure that holds information for queuing receivers after they de-register from a queue. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap indicating extra information about the deregistration. Zero or more flag bits ORed together: LBM_MSG_UMQ_DEREGISTRATION_COMPLETE_EX_FLAG_* (i.e. LBM_MSG_UMQ_DEREGISTRATION_COMPLETE_EX_FLAG_ULB)
lbm_uint_t | queue_id
| The Queue ID of the queue de-registering from.
char | queue [LBM_UMQ_MAX_QUEUE_STRLEN]
| The name of the queue.

## Detailed Description

Structure that holds information for queuing receivers after they de-register from a queue.

This structure is delivered to receiver callback lbm_rcv_cb_proc with lbm_msg_t::type set to LBM_MSG_UMQ_DEREGISTRATION_COMPLETE_EX. Cast the lbm_msg_t::data pointer to (lbm_msg_umq_deregistration_complete_ex_t *).

See lbm_msg_umq_deregistration_complete_ex_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h