UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_ume_store_entry_t_stct Struct Reference

Structure that holds information to configure a persistent Store. More...

`#include <lbm.h>`

## Data Fields
lbm_uint_t | ip_address
| The IP address of the UMP Store (network order)
lbm_ushort_t | tcp_port
| The TCP port of the Store (network order)
lbm_ushort_t | group_index
| The index of the group this UMP Store belongs to.
lbm_uint_t | registration_id
| The registration ID that should be used with this UMP Store for the source.
lbm_uint32_t | domain_id
| The domain ID of the Store.

## Detailed Description

Structure that holds information to configure a persistent Store.

Set by the ume_store (source) configuration option.

See lbm_ume_store_entry_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h