UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_src_event_umq_registration_complete_ex_t_stct Struct Reference

Structure that holds information for sources after registration is complete to all involved queue instances. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap indicating extra information about the registration. Zero or more flag bits ORed together: LBM_SRC_EVENT_UMQ_REGISTRATION_COMPLETE_EX_FLAG_* (i.e. LBM_SRC_EVENT_UMQ_REGISTRATION_COMPLETE_EX_FLAG_QUORUM)
lbm_uint_t | queue_id
| The Queue ID of the queue.
char | queue [LBM_UMQ_MAX_QUEUE_STRLEN]
| The name of the queue registered with.

## Detailed Description

Structure that holds information for sources after registration is complete to all involved queue instances.

This structure signals to the source successful source registration to a quorum of queue instances. Delivered as a source event LBM_SRC_EVENT_UMQ_REGISTRATION_COMPLETE_EX via callback lbm_src_cb_proc.

See lbm_src_event_umq_registration_complete_ex_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h