UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_umq_ulb_application_set_attr_t_stct Struct Reference

Structure that holds information to configure any of several ULB source's application set attributes. The attribute being set is determined by the configuration option. More...

`#include <lbm.h>`

## Data Fields
lbm_ushort_t | index
| Index of the Application Set.
union {
int d
| The integer value of the attribute.
lbm_ulong_t lu
| The unsigned long int value of the attribute.
} | value
| The value of the attribute.

## Detailed Description

Structure that holds information to configure any of several ULB source's application set attributes. The attribute being set is determined by the configuration option.

Set by the umq_ulb_application_set_events (source), umq_ulb_application_set_message_lifetime (source), umq_ulb_application_set_message_reassignment_timeout (source), umq_ulb_application_set_message_max_reassignments (source), umq_ulb_application_set_receiver_activity_timeout (source), umq_ulb_application_set_receiver_keepalive_interval (source), umq_ulb_application_set_assignment_function (source), umq_ulb_application_set_load_factor_behavior (source), and umq_ulb_application_set_round_robin_bias (source) configuration options.

See lbm_umq_ulb_application_set_attr_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h