UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_src_event_ume_registration_complete_ex_t_stct Struct Reference

Structure that holds information for sources after registration is complete to all involved Stores. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap indicating extra information about the registration. Zero or more flag bits ORed together: LBM_SRC_EVENT_UME_REGISTRATION_COMPLETE_EX_FLAG_* (i.e. LBM_SRC_EVENT_UME_REGISTRATION_COMPLETE_EX_FLAG_QUORUM)
lbm_uint_t | sequence_number
| The sequence number that will be the first sent.

## Detailed Description

Structure that holds information for sources after registration is complete to all involved Stores.

This structure signals to the source that the source has registered with a quorum of Stores and may proceed with sending messages. Delivered as source event LBM_SRC_EVENT_UME_REGISTRATION_COMPLETE_EX via callbacks lbm_src_cb_proc and lbm_ssrc_cb_proc.

See lbm_src_event_ume_registration_complete_ex_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h