UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
_Lbmmon__DROMonMsg__Stats__Portal__Peer__UDPSend Struct Reference

## Data Fields
ProtobufCMessage | base
uint64_t | msgs_sent
| Number of UDP datagrams sent.
uint64_t | bytes_sent
| Number of UDP datagram bytes sent.
uint64_t | nak_pckts_rcved
| Number of NAK packets received.
uint64_t | naks_rcved
| Number of individual NAKs received.
uint64_t | naks_ignored
| Number of NAKs ignored. NCF sent with reason code "ignored".
uint64_t | naks_shed
| Number of NAKs shed. NCF sent with reason code "shed".
uint64_t | naks_rx_delay_ignored
| Number of NAKs not yet processed due to rate limit. NCF sent with reason code "rx_delay".
uint64_t | rxs_sent
| Number of UDP datagrams retransmitted.
uint64_t | rx_bytes_sent
| Number of UDP datagram bytes retransmitted.

The documentation for this struct was generated from the following file:

- dro_mon.pb-c.h