UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbmpdm_timestamp_t Struct Reference

Structure to hold a timestamp value. More...

`#include <lbmpdm.h>`

## Data Fields
int32_t | tv_secs
int32_t | tv_usecs

## Detailed Description

Structure to hold a timestamp value.

The tv_secs is the number of seconds since the epoch. The tv_usecs is the additional microseconds since the epoch. and can range from -128 to 127.

## Field Documentation

int32_t lbmpdm_timestamp_t::tv_secs

Seconds since epoch

int32_t lbmpdm_timestamp_t::tv_usecs

Microseconds since last second

The documentation for this struct was generated from the following file:

- lbmpdm.h