UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
umestore_disk_dmon_stat_msg_t_stct Struct Reference

Message containing Store disk statistics.
( umestore_dmon_msg_hdr_t_stct::type == LBM_UMESTORE_DMON_MPG_DISK_STATS )
Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_UMESTORE_DMON_ANTIMAGIC. More...

`#include <umedmonmsgs.h>`

## Data Fields
umestore_dmon_msg_hdr_t | hdr
| Standard header common to all messages.
lbm_int64_t | max_offset
| The maximum size of the cache file, as configured by repository-disk-file-size-limit.
lbm_int64_t | num_ios_pending
| Number of disk writes the Store has submitted to the Operation System which have not yet completed.
lbm_int64_t | num_read_ios_pending
| Number of disk reads the Store has submitted to the Operation System which have not yet completed.
lbm_int64_t | offset
| The relative location on disk of where the message umestore_repo_dmon_stat_msg_t::contig_sqn+1 will be written.
lbm_int64_t | start_offset
| The relative location on disk of the first message, umestore_repo_dmon_stat_msg_t::trail_sqn.
lbm_uint32_t | dmon_topic_idx
| Identifying index number for the topic of this source, defined in an earlier message of type LBM_UMESTORE_DMON_MPG_STORE_TOPIC_CONFIG. See umestore_topic_dmon_config_msg_t_stct::dmon_topic_idx.
lbm_uint32_t | regid
| Registration ID used by the source to register.
lbm_uint16_t | store_idx
| Current Store number, starting with 0, counting each <store> element in the order configured.

## Detailed Description

Message containing Store disk statistics.
( umestore_dmon_msg_hdr_t_stct::type == LBM_UMESTORE_DMON_MPG_DISK_STATS )
Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_UMESTORE_DMON_ANTIMAGIC.

The documentation for this struct was generated from the following file:

- umedmonmsgs.h