UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_msg_fragment_info_t_stct Struct Reference

Structure that holds fragment information for UM messages when appropriate. More...

`#include <lbm.h>`

## Data Fields
lbm_uint_t | start_sequence_number
| The sequence number of the fragment that starts the message.
lbm_uint_t | offset
| The offset (in bytes) of this fragment from the message beginning.
lbm_uint_t | total_message_length
| The total length (in bytes) of the message this fragment is for.

## Detailed Description

Structure that holds fragment information for UM messages when appropriate.

To retrieve the UM-message fragment information held in this structure, it is typically necessary to call lbm_msg_retrieve_fragment_info().

See lbm_msg_fragment_info_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h