UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_resolver_service_entry_t_stct Struct Reference

Structure that holds information to configure a Resolver Service. More...

`#include <lbm.h>`

## Data Fields
lbm_uint_t | service_ip
| The IP address of the resolver service (network order)
lbm_ushort_t | service_port
| The port configured on the resolver service. (network order)
lbm_ipv4_address_mask_t | iface
| Interface to be used.
lbm_ushort_t | source_port
| The source port to be used (network order).

## Detailed Description

Structure that holds information to configure a Resolver Service.

Set by the resolver_service (context) configuration option.

For more information on the Resolver Service, see TCP TR.

See lbm_resolver_service_entry_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h