UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_resolver_event_advertisement_t_stct Struct Reference

Advertisement event structure (for UM internal use only). More...

`#include <lbm.h>`

## Data Fields
lbm_uint32_t | flags
| Bitmap indicating extra information about the advertisement. Zero or more flag bits ORed together: LBM_RESOLVER_EVENT_ADVERTISEMENT_FLAGS_* (i.e. LBM_RESOLVER_EVENT_ADVERTISEMENT_FLAGS_LJ, LBM_RESOLVER_EVENT_ADVERTISEMENT_FLAGS_UME, LBM_RESOLVER_EVENT_ADVERTISEMENT_FLAGS_UMQ, LBM_RESOLVER_EVENT_ADVERTISEMENT_FLAGS_ULB, LBM_RESOLVER_EVENT_ADVERTISEMENT_FLAGS_EVC)
char | topic_string [LBM_MSG_MAX_TOPIC_LEN]
| Source topic string.
char | transport_string [LBM_MSG_MAX_SOURCE_LEN]
| Source string.
lbm_uint32_t | topic_index
| Topic index within transport session.
lbm_uint32_t | source_domain_id
| Domain ID of originating source.
lbm_uint8_t | otid [LBM_OTID_BLOCK_SZ]
| Globally unique identifier of originating source.
lbm_uint32_t | source_type
| Type of source.

## Detailed Description

Advertisement event structure (for UM internal use only).

The documentation for this struct was generated from the following file:

- lbm.h