UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
umestore_rcv_dmon_stat_msg_t_stct Struct Reference

Message containing Store receiver statistics.
( umestore_dmon_msg_hdr_t_stct::type == LBM_UMESTORE_DMON_MPG_RCV_STATS )
Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_UMESTORE_DMON_ANTIMAGIC. More...

`#include <umedmonmsgs.h>`

## Data Fields
umestore_dmon_msg_hdr_t | hdr
| Standard header common to all messages.
lbm_uint32_t | dmon_topic_idx
| Identifying index number for the topic of this source, defined in an earlier message of type LBM_UMESTORE_DMON_MPG_STORE_TOPIC_CONFIG. See umestore_topic_dmon_config_msg_t_stct::dmon_topic_idx.
lbm_uint32_t | regid
| Registration ID used by the receiver to register.
lbm_uint32_t | high_ack_sqn
| The last message sequence number the receiver acknowledged.
lbm_uint16_t | store_idx
| Current Store number, starting with 0, counting each <store> element in the order configured.
lbm_uint16_t | flags
| Bit map of flags indicating various characteristics and current states of the Store. Possible bits: UMESTORE_DMON_RCV_FLAG_FIRST_ACK, UMESTORE_DMON_RCV_FLAG_OOD, UMESTORE_DMON_RCV_FLAG_CAPABILITY_QC, UMESTORE_DMON_RCV_FLAG_SHUTTING_DOWN, UMESTORE_DMON_RCV_FLAG_DEREGISTERING, UMESTORE_DMON_RCV_FLAG_RPP, UMESTORE_DMON_RCV_FLAG_RPP, UMESTORE_DMON_RCV_FLAG_RPP_IS_NON_BLOCKING, UMESTORE_DMON_RCV_FLAG_KEEPALIVES_DISABLED.

## Detailed Description

Message containing Store receiver statistics.
( umestore_dmon_msg_hdr_t_stct::type == LBM_UMESTORE_DMON_MPG_RCV_STATS )
Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_UMESTORE_DMON_ANTIMAGIC.

The documentation for this struct was generated from the following file:

- umedmonmsgs.h