UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_src_event_ume_registration_ex_t_stct Struct Reference

Structure that holds Store registration information for the UMP source in an extended form. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap indicating extra information about the registration. Zero or more flag bits ORed together: LBM_SRC_EVENT_UME_REGISTRATION_SUCCESS_EX_FLAG_* (i.e. LBM_SRC_EVENT_UME_REGISTRATION_SUCCESS_EX_FLAG_OLD, LBM_SRC_EVENT_UME_REGISTRATION_SUCCESS_EX_FLAG_NOACKS, LBM_SRC_EVENT_UME_REGISTRATION_SUCCESS_EX_FLAG_RPP)
lbm_uint_t | registration_id
| The registration ID for the source.
lbm_uint_t | sequence_number
| The sequence number for the source to use as reported by the Store.
lbm_ushort_t | store_index
| the Store index of the Store involved
char | store [LBM_UME_MAX_STORE_STRLEN]
| the Store that was registered with

## Detailed Description

Structure that holds Store registration information for the UMP source in an extended form.

This structure signals to the source successful registration of a source with a Store. It indicates initial staring information related to that Store. Delivered as a source event LBM_SRC_EVENT_UME_REGISTRATION_SUCCESS_EX via callbacks lbm_src_cb_proc and lbm_ssrc_cb_proc.

See lbm_src_event_ume_registration_ex_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h