UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
tnwg_rm_stat_grp_local_info_t_stct Struct Reference

Structure containing high-level information about this UM Router's (DRO) view of the current topology. Used by tnwg_rm_stat_grp_msg_t. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC. More...

`#include <tnwgdmonmsgs.h>`

## Data Fields
char | gateway_name [TNWG_DSTAT_MAX_GATEWAY_NAME_LEN]
| Name of this DRO.
uint64_t | gateway_id
| DRO id.
uint32_t | topology_signature
| Topology signature.
uint32_t | recalc_duration_sec
| Recalc duration sec.
uint32_t | recalc_duration_usec
| Recalc duration usec.
uint32_t | graph_version
| Graph version.
uint16_t | self_version
| Self version.
uint16_t | gateway_count
| DRO count.
uint16_t | trd_count
| Trd count.

## Detailed Description

Structure containing high-level information about this UM Router's (DRO) view of the current topology. Used by tnwg_rm_stat_grp_msg_t. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC.

The documentation for this struct was generated from the following file:

- tnwgdmonmsgs.h