UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_rcv_src_notification_func_t_stct Struct Reference

Structure that holds the receiver application functions when configuring callbacks when sources are subscribed or unsubscribed. More...

`#include <lbm.h>`

## Data Fields
lbm_rcv_src_notification_create_function_cb | create_func
| Function pointer for application callback when delivery controller is created.
lbm_rcv_src_notification_delete_function_cb | delete_func
| Function pointer for application callback when delivery controller is deleted.
void * | clientd
| Client data to be passed to the callback.

## Detailed Description

Structure that holds the receiver application functions when configuring callbacks when sources are subscribed or unsubscribed.

Set by the the source_notification_function (receiver) configuration option.

See lbm_rcv_src_notification_func_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h