UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_src_event_wakeup_t_stct Struct Reference

Structure that holds source wakeup event data. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap indicating which context-level sources are now unblocked. Zero or more flag bits ORed together: LBM_SRC_EVENT_WAKEUP_FLAG_* (i.e. LBM_SRC_EVENT_WAKEUP_FLAG_NORMAL, LBM_SRC_EVENT_WAKEUP_FLAG_MIM, LBM_SRC_EVENT_WAKEUP_FLAG_UIM, LBM_SRC_EVENT_WAKEUP_FLAG_REQUEST, LBM_SRC_EVENT_WAKEUP_FLAG_RESPONSE)

## Detailed Description

Structure that holds source wakeup event data.

This structure signals to the source that the application may resume sending. This source had previously returned LBM_EWOULDBLOCK. Delivered as a source event LBM_SRC_EVENT_WAKEUP via callbacks lbm_context_src_cb_proc and lbm_src_cb_proc.

See lbm_src_event_wakeup_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h