UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_context_event_umq_registration_ex_t_stct Struct Reference

Structure that holds queue registration information for the UMQ context in an extended form. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap set of flags reserved for future use. Currently set to 0.
lbm_umq_regid_t | registration_id
| Registration ID used for the registration.
lbm_uint_t | queue_id
| The Queue ID of the queue.
lbm_uint_t | queue_instance_index
| The index of the instance of the queue registered with.
char | queue_instance [LBM_UME_MAX_STORE_STRLEN]
| The instance of the queue registered with.
char | queue [LBM_UMQ_MAX_QUEUE_STRLEN]
| The name of the queue registered with.

## Detailed Description

Structure that holds queue registration information for the UMQ context in an extended form.

A structure used with UMQ receivers and sources to indicate successful context registration with an instance of the queue.

See lbm_context_event_umq_registration_ex_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h