UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_umm_info_t_stct Struct Reference

Structure for specifying UMM daemon connection options. More...

`#include <lbm.h>`

## Data Fields
char | username [LBM_UMM_USER_NAME_LENGTH_MAX]
| The UMM user name.
char | password [LBM_UMM_PASSWORD_LENGTH_MAX]
| The UMM user password.
char | appname [LBM_UMM_APP_NAME_LENGTH_MAX]
| The UMM application name.
char | servers [LBM_UMM_NUM_SERVERS_MAX][LBM_UMM_SERVER_LENGTH_MAX]
| The list of UMM daemons in ip:port string format. Connections are tried in a round robin fashion, starting with index 0. Only the first contiguous set of non-blank entries are considered.
lbm_uint32_t | flags
| Bitmap indicating extra information about the UMM connection. Zero or more flag bits ORed together: LBM_UMM_INFO_FLAGS_* (i.e. LBM_UMM_INFO_FLAGS_USE_SSL)
char * | cert_file
| Path to a pem-encoded certificate file. If non-NULL, SSL is enabled and is used to validate the the UMM daemon certificate.
char * | cert_file_password
| Certificate file password. Required only if certificate file is password-protected.

## Detailed Description

Structure for specifying UMM daemon connection options.

See lbm_umm_info_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h