UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
tnwg_rm_stat_grp_othergw_neighbor_t_stct Struct Reference

Structure containing this UM Router's (DRO) view of a remote DRO's portal information. Used by tnwg_rm_stat_grp_msg_t. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC. More...

`#include <tnwgdmonmsgs.h>`

## Data Fields
uint64_t | node_id
| Node ID.
uint32_t | domain_or_gateway
| 0 for domain, 1 for DRO.
uint32_t | ingress_cost
| Cost from this node_id to the owning neighbor_info's node_id.

## Detailed Description

Structure containing this UM Router's (DRO) view of a remote DRO's portal information. Used by tnwg_rm_stat_grp_msg_t. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC.

The documentation for this struct was generated from the following file:

- tnwgdmonmsgs.h