UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_msg_ume_registration_complete_ex_t_stct Struct Reference

Structure that holds information for receivers after registration is complete to all involved Stores. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap indicating extra information about the registration. Zero or more flag bits ORed together: LBM_MSG_UME_REGISTRATION_COMPLETE_EX_FLAG_* (i.e. LBM_MSG_UME_REGISTRATION_COMPLETE_EX_FLAG_QUORUM, LBM_MSG_UME_REGISTRATION_COMPLETE_EX_FLAG_RXREQMAX, LBM_MSG_UME_REGISTRATION_COMPLETE_EX_FLAG_SRC_SID)
lbm_uint_t | sequence_number
| The sequence number that will be the first requested.
lbm_uint64_t | src_session_id
| The session ID for the source.

## Detailed Description

Structure that holds information for receivers after registration is complete to all involved Stores.

This structure is delivered to the application by the receiver callback lbm_rcv_cb_proc with event lbm_msg_t::type LBM_MSG_UME_REGISTRATION_COMPLETE_EX. The lbm_msg_t::data pointer should be cast to (lbm_msg_ume_registration_complete_ex_t *).

See lbm_msg_ume_registration_complete_ex_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h