UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_rcv_transport_stats_broker_t_stct Struct Reference

Structure that holds message statistics for receiver BROKER transports. More...

`#include <lbm.h>`

## Data Fields
lbm_ulong_t | msgs_rcved
| Number of BROKER messages received. Messages received from a broker always map to an lbm_msg_t unless there is an error. (Cumulative)
lbm_ulong_t | bytes_rcved
| Number of BROKER message bytes received. This does not include overhead for the AMQP protocol. (Cumulative)

## Detailed Description

Structure that holds message statistics for receiver BROKER transports.

Note that when stats are sampled, the fields in the structure are not necessarily from the same instant in time. The structure might be updated concurrently with it being sampled, and while each structure field is atomically read, the field values can be skewed slightly across time.

See lbm_rcv_transport_stats_broker_t_stct for field definitions.

Cumulative vs Snapshot

These UM statistics are cumulative. For example, msgs_rcved starts at zero and grows over time as more and more messages are sent.

The documentation for this struct was generated from the following file:

- lbm.h