UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
tnwg_pcfg_stat_grp_rec_hdr_t_stct Struct Reference

Structure containing portal configuration information. Used by tnwg_pcfg_stat_grp_msg_t. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC. More...

`#include <tnwgdmonmsgs.h>`

## Data Fields
uint32_t | portal_num
| Portal number.
uint32_t | portal_type
| Portal type: TNWG_DSTAT_Portal_Type_Peer TNWG_DSTAT_Portal_Type_Endpoint.
uint32_t | num_options
| Number of options stored in tnwg_pcfg_stat_grp_msg_t_stct::data.
uint32_t | padding
| Name of portal.
char | portal_name [TNWG_DSTAT_MAX_PORTAL_NAME_LEN]
char | attr_type [MAX_ATTR_TYPE_NAME_LEN]
| Type of options stored in tnwg_pcfg_stat_grp_msg_t_stct::data.

## Detailed Description

Structure containing portal configuration information. Used by tnwg_pcfg_stat_grp_msg_t. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC.

The documentation for this struct was generated from the following file:

- tnwgdmonmsgs.h