UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_msg_ume_deregistration_ex_t_stct Struct Reference

Structure that holds Store deregistration information for the UM receiver after a successful deregistration. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap indicating extra information about the deregistration. Zero or more flag bits ORed together: LBM_MSG_UME_DEREGISTRATION_SUCCESS_EX_FLAG_* (i.e. LBM_MSG_UME_DEREGISTRATION_SUCCESS_EX_FLAG_RPP)
lbm_uint_t | src_registration_id
| The registration ID for the source.
lbm_uint_t | rcv_registration_id
| The registration ID for the receiver.
lbm_uint_t | sequence_number
| The sequence number for the receiver to end at as reported by the Store.
lbm_ushort_t | store_index
| the Store index of the Store involved
char | store [LBM_UME_MAX_STORE_STRLEN]
| the Store that was registered with

## Detailed Description

Structure that holds Store deregistration information for the UM receiver after a successful deregistration.

This structure is delivered to receiver callback lbm_rcv_cb_proc with lbm_msg_t::type set to LBM_MSG_UME_DEREGISTRATION_SUCCESS_EX. Cast the lbm_msg_t::data pointer to (lbm_msg_ume_deregistration_ex_t *).

See lbm_msg_ume_deregistration_ex_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h