UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_src_event_umq_message_id_info_t_stct Struct Reference

Structure that holds Message ID information for a message sent by a sending UMQ application. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap set of flags reserved for future use. Currently set to 0.
lbm_umq_msgid_t | msg_id
| Message ID for the message sent.
void * | msg_clientd
| The clientd pointer passed in for the message.

## Detailed Description

Structure that holds Message ID information for a message sent by a sending UMQ application.

See also
  lbm_src_send_ex() A structure used with UMQ sending applications that informs the application of the UMQ Message ID used with a message.

See lbm_src_event_umq_message_id_info_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h