UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_src_event_ume_deregistration_ex_t_stct Struct Reference

Structure that holds Store deregistration information for the UMP source in an extended form. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap set of flags reserved for future use. Currently set to 0.
lbm_uint32_t | registration_id
| The registration ID for the source.
lbm_uint_t | sequence_number
| The sequence number of the last message stored for the source as reported by the Store.
lbm_ushort_t | store_index
| the Store index of the Store involved.
char | store [LBM_UME_MAX_STORE_STRLEN]
| the Store that was registered with.

## Detailed Description

Structure that holds Store deregistration information for the UMP source in an extended form.

A structure used with UMP sources to indicate successful deregistration (extended form).

See lbm_src_event_ume_deregistration_ex_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h