UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_hf_sequence_number_t_stct Union Reference

Structure to hold a hot failover sequence number. More...

`#include <lbm.h>`

## Data Fields
lbm_uint32_t | u32
| 32 bit hot failover sequence number
lbm_uint64_t | u64
| 64 bit hot failover sequence number

## Detailed Description

Structure to hold a hot failover sequence number.

The documentation for this union was generated from the following file:

- lbm.h