UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
tnwg_pcfg_stat_grp_msg_t_stct Struct Reference

Message containing memory allocation statistics.
( tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_PORTCFG )
Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC. More...

`#include <tnwgdmonmsgs.h>`

## Data Fields
tnwg_dstat_msg_hdr_t | msghdr
| Standard header common to all messages.
tnwg_pcfg_stat_grp_rec_hdr_t | rechdr
| Structure containing portal configuration information.
char | data
| String data containing portal configuration attributes. The number of strings is given by tnwg_pcfg_stat_grp_msg_t_stct::rechdr->num_options. See DRO Daemon Statistics String Buffers for more information.

## Detailed Description

Message containing memory allocation statistics.
( tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_PORTCFG )
Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC.

The documentation for this struct was generated from the following file:

- tnwgdmonmsgs.h