UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_srp_repo_rcvr_t_stct Struct Reference

Receiver state information, retrieved by lbm_srp_get_repo_state() via lbm_srp_repo_t::rcvs. More...

`#include <umeprofile.h>`

## Data Fields
lbm_uint32_t | regid
| registration identifier
lbm_uint32_t | sqn
| high ack sequence number
lbm_uint16_t | store_id
| store identifier
lbm_uint16_t | rcv_port
| receiver IP port
lbm_uint32_t | rcv_addr
| receiver IP address
lbm_uint32_t | transport_idx
| receiver transport index
lbm_uint32_t | topic_idx
| topic index
lbm_uint64_t | sid
| receiver session identifier
lbm_uint16_t | flags
| flags
lbm_uint8_t | otid [LBM_OTID_BLOCK_SZ]
| originating transport identifier
lbm_uint8_t | ctxinst [LBM_CONTEXT_INSTANCE_BLOCK_SZ]
| context instance block
lbm_uint32_t | rcv_domain_id
| receive domain identifier
lbm_ulong_t | considered_activity_tmo
| considered activity timeout
lbm_ulong_t | considered_state_lifetime
| considered state lifetime

## Detailed Description

Receiver state information, retrieved by lbm_srp_get_repo_state() via lbm_srp_repo_t::rcvs.

The documentation for this struct was generated from the following file:

- umeprofile.h