UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
tnwg_dstat_portalstats_msg_t_stct Struct Reference

Message containing portal statistics.
( tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_PORTSTAT )
This message can have different lengths, depending on which element of the union tnwg_portalstats_dstat_record_t_stct::ptype is selected, based on the value of tnwg_dstat_record_hdr_t_stct::portal_type. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC. More...

`#include <tnwgdmonmsgs.h>`

## Data Fields
tnwg_dstat_msg_hdr_t | msghdr
| Standard header common to all messages.
tnwg_dstat_record_hdr_t | rechdr
| General information about this portal.
tnwg_portalstats_dstat_record_t | record
| Type-specific information about this portal.

## Detailed Description

Message containing portal statistics.
( tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_PORTSTAT )
This message can have different lengths, depending on which element of the union tnwg_portalstats_dstat_record_t_stct::ptype is selected, based on the value of tnwg_dstat_record_hdr_t_stct::portal_type. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC.

The documentation for this struct was generated from the following file:

- tnwgdmonmsgs.h