UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_umq_msgid_t_stct Struct Reference

Structure that holds information for UMQ messages that allows the message to be identified uniquely. More...

`#include <lbm.h>`

## Data Fields
lbm_umq_regid_t | regid
| The Registration ID of the original source context of the message.
lbm_uint64_t | stamp
| The stamp of the message that indicates the individual message from the given source context.

## Detailed Description

Structure that holds information for UMQ messages that allows the message to be identified uniquely.

See also
  lbm_umq_regid_t A structure used with UMQ messages to identify a message uniquely.

See lbm_umq_msgid_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h