UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
ume_liveness_receiving_context_t_stct Struct Reference

Structure that holds the information about a receiving context. More...

`#include <lbm.h>`

## Data Fields
lbm_uint64_t | regid
| Registration ID.
lbm_uint64_t | session_id
| Session ID.
int | flag
| Flag: Bitmap of flag bits ORed together. Bits are: LBM_UME_LIVENESS_RECEIVER_UNRESPONSIVE_FLAG_* (i.e. LBM_UME_LIVENESS_RECEIVER_UNRESPONSIVE_FLAG_TMO, LBM_UME_LIVENESS_RECEIVER_UNRESPONSIVE_FLAG_EOF)

## Detailed Description

Structure that holds the information about a receiving context.

A structure used to hold a receiving context's user rcv regid and session id. Source contexts use this information to track receiver liveness.

See ume_liveness_receiving_context_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h