UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_msg_channel_info_t_stct Struct Reference

Structure that represents UMS Spectrum channel information. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap indicating extra channel information. Zero or more flag bits ORed together: LBM_MSG_FLAG_NUMBERED_CHANNEL.
lbm_uint32_t | channel_number
| Channel number in the range 0-4294967295.

## Detailed Description

Structure that represents UMS Spectrum channel information.

This channel information assigns a channel designator to individual messages. Receivers may use this channel designator to filter messages or direct them to specific callbacks on a per-channel basis.

See lbm_msg_channel_info_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h