UM Java API 6.17.1

- Main Page
- Related Pages
- Classes

- Class List
- Class Hierarchy
- Class Members

Public Member Functions | List of all members
com.latencybusters.lbm.UMQSourceEventULBReceiverInfo Class Reference
Inheritance diagram for com.latencybusters.lbm.UMQSourceEventULBReceiverInfo:

## Public Member Functions
| UMQSourceEventULBReceiverInfo (int flags, long regId, long assignId, long appSetIdx, String receiver) throws LBMEInvalException
int | flags ()
long | registrationId ()
long | assignmentId ()
long | applicationSetIndex ()
String | receiver ()

## Detailed Description

UMQ ULB Receiver Info class. This info object is both delivered with a source event and acts as a base class for other ULB source events. In both cases, this object holds information about a ULB receiver.

Since
  UMQ 1.1

## Constructor & Destructor Documentation

com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.UMQSourceEventULBReceiverInfo | ( | int | flags,
|  | long | regId,
|  | long | assignId,
|  | long | appSetIdx,
|  | String | receiver
| ) |  | throws LBMEInvalException

Creates a UMQSourceEventULBReceiverInfo object and initializes fields to the supplied values.

Parameters

  flags | Informational flags.
  regId | Registration ID of the receiver.
  assignId | The Assignment ID of the receiver.
  appSetIdx | The application set index the receiver is in.
  receiver | The receivers immediate message target string.

Exceptions

  LBMEInvalException | An invalid parameter was specified.

Since
  UMQ 1.1

References com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.flags(), and com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.receiver().

## Member Function Documentation

long com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.applicationSetIndex | ( |  | ) |

Get Application Set index for the receiver associated with this info object.

Returns
  Application Set index for the receiver associated with this info object.

Since
  UMQ 1.1

long com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.assignmentId | ( |  | ) |

Get Assignment ID for the receiver associated with this info object.

Returns
  Assignment ID of the receiver associated with this info object.

Since
  UMQ 1.1

int com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.flags | ( |  | ) |

Get informational flags for this info object.

Returns
  Flags.

Since
  UMQ 1.1

Referenced by com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.receiver(), com.latencybusters.lbm.UMQSourceEventULBMessageInfo.UMQSourceEventULBMessageInfo(), and com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.UMQSourceEventULBReceiverInfo().

String com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.receiver | ( |  | ) |

Get immediate message target string for the receiver associated with this info object.

Returns
  Immediate message target string for the receiver associated with this info object.

Since
  UMQ 1.1

References com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.flags().

Referenced by com.latencybusters.lbm.UMQSourceEventULBMessageInfo.UMQSourceEventULBMessageInfo(), and com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.UMQSourceEventULBReceiverInfo().

long com.latencybusters.lbm.UMQSourceEventULBReceiverInfo.registrationId | ( |  | ) |

Get Registration ID for the receiver associated with this info object.

Returns
  Registration ID of the receiver associated with this info object.

Since
  UMQ 1.1

The documentation for this class was generated from the following file:

- UMQSourceEventULBReceiverInfo.java