UM Java API 6.17.1

- Main Page
- Related Pages
- Classes

- Class List
- Class Hierarchy
- Class Members

Public Member Functions | List of all members
com.latencybusters.lbm.UMERecoverySequenceNumberCallback Interface Reference

## Public Member Functions
int | setRecoverySequenceNumberInfo (Object cbArg, UMERecoverySequenceNumberCallbackInfo cbInfo)

## Detailed Description

Interface for setting receiver recovery sequence number information. (UME only.)

## Member Function Documentation

int com.latencybusters.lbm.UMERecoverySequenceNumberCallback.setRecoverySequenceNumberInfo | ( | Object | cbArg,
|  | UMERecoverySequenceNumberCallbackInfo | cbInfo
| ) |  |

Callback method for getting information about recovery sequence numbers and setting the desired low sequence number. Call UMERecoverySequenceNumberCallbackInfo#setLowSequenceNumber(long) in this callback before returning to set the desired low sequence number.

Parameters

  cbArg | Client-supplied callback object.
  cbInfo | Information about recovery sequence numbers (low, high, etc.).

Returns
  0 on success, -1 on error.

Since
  UME 2.0

The documentation for this interface was generated from the following file:

- UMERecoverySequenceNumberCallback.java