UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
tnwg_dstat_gatewaycfg_msg_t_stct Struct Reference

Message containing DRO configuration information.
( tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_GATEWAYCFG )
Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC. More...

`#include <tnwgdmonmsgs.h>`

## Data Fields
tnwg_dstat_msg_hdr_t | msghdr
| Standard header common to all messages.
char | data
| String data containing DRO configuration. See DRO Daemon Statistics String Buffers.

## Detailed Description

Message containing DRO configuration information.
( tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_GATEWAYCFG )
Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC.

The documentation for this struct was generated from the following file:

- tnwgdmonmsgs.h