UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_ipv4_address_mask_t_stct Struct Reference

Structure that holds an IPv4 address and a CIDR style netmask. More...

`#include <lbm.h>`

## Data Fields
lbm_uint_t | addr
| IPv4 address in network byte order, as might be returned from inet_aton().
int | bits
| Number of leading 1's in the netmask. E.g. the value 28 represents a netmask of 0xFFFFFFF0.

## Detailed Description

Structure that holds an IPv4 address and a CIDR style netmask.

Used with various configuration options that require an IP address.

See lbm_ipv4_address_mask_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h