UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
tnwg_rm_stat_grp_msg_t_stct Struct Reference

Message containing routing information.
( tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_RM_LOCAL,
TNWG_DSTATTYPE_RM_PORTAL, TNWG_DSTATTYPE_RM_OTHERGW,
TNWG_DSTATTYPE_RM_OTHERGW_NBR )
This message can have different lengths, depending on which element of the union `msgtype` is selected, based on the message type in tnwg_dstat_msg_hdr_t_stct::type. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC. More...

`#include <tnwgdmonmsgs.h>`

## Data Fields
tnwg_dstat_msg_hdr_t | msghdr
| Standard header common to all messages.
union {
tnwg_rm_stat_grp_local_info_t local
| Use when tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_RM_LOCAL.
tnwg_rm_stat_grp_portal_info_t portal
| Use when tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_RM_PORTAL.
tnwg_rm_stat_grp_othergw_info_t othergw
| Use when tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_RM_OTHERGW.
tnwg_rm_stat_grp_othergw_neighbor_t neighbor
| Use when tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_RM_OTHERGW_NBR.
} | msgtype
| union containing the different types of route information messages.

## Detailed Description

Message containing routing information.
( tnwg_dstat_msg_hdr_t_stct::type == TNWG_DSTATTYPE_RM_LOCAL,
TNWG_DSTATTYPE_RM_PORTAL, TNWG_DSTATTYPE_RM_OTHERGW,
TNWG_DSTATTYPE_RM_OTHERGW_NBR )
This message can have different lengths, depending on which element of the union `msgtype` is selected, based on the message type in tnwg_dstat_msg_hdr_t_stct::type. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC.

The documentation for this struct was generated from the following file:

- tnwgdmonmsgs.h