UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_umq_ulb_receiver_type_entry_t_stct Struct Reference

Structure that holds ULB queue information to configure an application set. More...

`#include <lbm.h>`

## Data Fields
lbm_ulong_t | id
| Receiver Type ID.
lbm_ushort_t | application_set_index
| Index of the Application Set the receiver is in.

## Detailed Description

Structure that holds ULB queue information to configure an application set.

Set by the umq_ulb_application_set (source) configuration option.

See lbm_umq_ulb_receiver_type_entry_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h