UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_src_transport_stats_lbtrdma_t_stct Struct Reference

DEPRECATED, do not use. lbt-rdma is no longer supported. More...

`#include <lbm.h>`

## Data Fields
lbm_ulong_t | num_clients
| Number of receiver transports that are currently connected to this source transport.
lbm_ulong_t | msgs_sent
| Number of LBT-RDMA datagrams sent. Depending on batching settings, a single LBT-RDMA datagram may contain one or more messages, or a fragment of a larger message. With LBT-RDMA, larger messages are split into fragment sizes limited by configuration option transport_lbtrdma_datagram_max_size (context) (default 4KB).
lbm_ulong_t | bytes_sent
| Number of LBT-RDMA datagram bytes sent, i.e., the total of lengths of all LBT-RDMA packets including UM header information.

## Detailed Description

DEPRECATED, do not use. lbt-rdma is no longer supported.

Deprecated:
  do not use. LBT-RDMA is no longer supported.

The documentation for this struct was generated from the following file:

- lbm.h