UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_rcv_topic_stats_t_stct Struct Reference

Structure that holds statistics for a receiver topic. More...

`#include <lbm.h>`

## Data Fields
char | topic [LBM_MSG_MAX_TOPIC_LEN]
| Topic for the receiver. THIS FIELD IS UNSUPPORTED.
lbm_uint32_t | flags
| Flags for the receiver. THIS FIELD IS UNSUPPORTED.
char | source [LBM_MSG_MAX_SOURCE_LEN]
| Source string for a transport joined by the receiver. THIS FIELD IS UNSUPPORTED.
lbm_uint8_t | otid [LBM_OTID_BLOCK_SZ]
| Originating transport ID for a transport joined by the receiver. THIS FIELD IS UNSUPPORTED.
lbm_uint32_t | topic_idx
| Topic index for a transport joined by the receiver. THIS FIELD IS UNSUPPORTED.
lbm_uint64_t | timestamp_sec
| Timestamp seconds of when a transport was joined by the receiver. THIS FIELD IS UNSUPPORTED.
lbm_uint64_t | timestamp_usec
| Timestamp microseconds of when a transport was joined by the receiver. THIS FIELD IS UNSUPPORTED.

## Detailed Description

Structure that holds statistics for a receiver topic.

THIS STRUCTURE IS UNSUPPORTED.

The documentation for this struct was generated from the following file:

- lbm.h