UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_src_event_ume_ack_info_t_stct Struct Reference

Structure that holds ACK information for a given message. More...

`#include <lbm.h>`

## Data Fields
lbm_uint_t | sequence_number
| The sequence number of the message that is being acknowledged.
lbm_uint_t | rcv_registration_id
| The registration ID for the receiver.
void * | msg_clientd
| The clientd pointer passed in for the message.

## Detailed Description

Structure that holds ACK information for a given message.

Deprecated:
  This event is no longer generated by UM. Use lbm_src_event_ume_ack_ex_info_t_stct instead.

The documentation for this struct was generated from the following file:

- lbm.h