UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_ucast_resolver_entry_t_stct Struct Reference

Structure that holds information to configure a unicast resolver daemon. More...

`#include <lbm.h>`

## Data Fields
lbm_ipv4_address_mask_t | iface
| Interface to be used.
lbm_uint_t | resolver_ip
| The IP address of the unicast resolver daemon (network order)
lbm_ushort_t | source_port
| The source port. Use 0 to indicate that the port should come from the range resolver_unicast_port_low (context) ... resolver_unicast_port_high (context). (network order)
lbm_ushort_t | destination_port
| The port configured on the unicast resolver daemon. (network order)

## Detailed Description

Structure that holds information to configure a unicast resolver daemon.

Set by the resolver_unicast_daemon (context) configuration option.

See lbm_ucast_resolver_entry_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h