UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_transport_broker_entry_t_stct Struct Reference

Structure that holds IP and Port to configure the broker. More...

`#include <lbm.h>`

## Data Fields
lbm_uint_t | broker_ip
| The IP address of the broker (network order)
lbm_ushort_t | broker_port
| The port of the broker. (network order)
lbm_ipv4_address_mask_t | iface
| Future: not currently implemented. Interface to be used.
lbm_ushort_t | source_port
| Future: not currently implemented. The source port to be used (network order).

## Detailed Description

Structure that holds IP and Port to configure the broker.

Set by the broker (context) configuration option.

See Queuing for information on brokered queuing.

See lbm_transport_broker_entry_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h