UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_ume_rcv_recovery_info_ex_func_t_stct Struct Reference

Structure that holds the application function to configure the callback for recovery sequence number information, extended form. More...

`#include <lbm.h>`

## Data Fields
lbm_ume_rcv_recovery_info_ex_function_cb | func
| Function pointer for application callback function.
void * | clientd
| Client data to be passed to the callback.

## Detailed Description

Structure that holds the application function to configure the callback for recovery sequence number information, extended form.

Set by the ume_recovery_sequence_number_info_function (receiver) configuration option.

See lbm_ume_rcv_recovery_info_ex_func_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h