UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_iovec_t_stct Struct Reference

Structure, struct iovec compatible, that holds information about buffers used for vectored sends. More...

`#include <lbm.h>`

## Data Fields
char * | iov_base
| Pointer to a segment of application data.
size_t | iov_len
| Number of bytes in this segment.

## Detailed Description

Structure, struct iovec compatible, that holds information about buffers used for vectored sends.

UM replacement for struct iovec for portability. See lbm_src_sendv(), lbm_src_sendv_ex(), etc.

See lbm_iovec_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h