UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
tnwg_rm_stat_grp_portal_info_t_stct Struct Reference

Structure containing routing information specific to a particular portal. Used by tnwg_rm_stat_grp_msg_t. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC. More...

`#include <tnwgdmonmsgs.h>`

## Data Fields
uint64_t | node_or_adjacent_id
| ID of adjacent DRO (for `type` == TNWG_DSTAT_Portal_Type_Peer), or Topic Resolution Domain ID (for `type` == TNWG_DSTAT_Portal_Type_Endpoint).
uint32_t | type
| Portal type: TNWG_DSTAT_Portal_Type_Peer TNWG_DSTAT_Portal_Type_Endpoint.
uint32_t | index
| Portal index.
uint32_t | ingress_cost
| Cost.
uint32_t | recalc_duration_sec
| Recalc duration sec.
uint32_t | recalc_duration_usec
| Recalc duration usec.
uint32_t | proxy_rec_recalc_duration_sec
| Proxy rec recalc duration sec.
uint32_t | proxy_rec_recalc_duration_usec
| Proxy rec recalc duration usec.
char | portal_name [TNWG_DSTAT_MAX_PORTAL_NAME_LEN]
| Portal name.

## Detailed Description

Structure containing routing information specific to a particular portal. Used by tnwg_rm_stat_grp_msg_t. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC.

The documentation for this struct was generated from the following file:

- tnwgdmonmsgs.h