UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_ume_rcv_regid_ex_func_info_t_stct Struct Reference

Structure that holds information for UMP receiver registration ID application callbacks. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap set of flags reserved for future use. Currently set to 0.
lbm_uint_t | src_registration_id
| The registration ID for the source.
lbm_ushort_t | store_index
| the Store index of the Store involved
void * | source_clientd
| The per-source clientd value for the source set by the lbm_rcv_src_notification_create_function_cb callback.
char | source [LBM_MSG_MAX_SOURCE_LEN]
| The source for the registration ID.
char | store [LBM_UME_MAX_STORE_STRLEN]
| the Store involved

## Detailed Description

Structure that holds information for UMP receiver registration ID application callbacks.

A structure used with UMP receiver registration ID callbacks to pass in information.

See also
  lbm_ume_rcv_regid_func_t

See lbm_ume_rcv_regid_ex_func_info_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h