UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbmmon_packet_attributes_t_stct Struct Reference

## Data Fields
lbm_ushort_t | mPacketAttributesMagic
uint64_t | mFlags
lbm_uint_t | mAddress
time_t | mTimestamp
lbm_ushort_t | mModuleID
lbm_ushort_t | mSourceFlag
char | mApplicationSourceID [LBM_MSG_MAX_TOPIC_LEN]
lbm_uint64_t | mObjectID
lbm_uint64_t | mProcessID
unsigned char | mContextInstance [LBM_CONTEXT_INSTANCE_BLOCK_SZ]
lbm_uint32_t | mDomainID

## Field Documentation

lbm_uint_t lbmmon_packet_attributes_t_stct::mAddress

The sender IPv4 address in network order.

char lbmmon_packet_attributes_t_stct::mApplicationSourceID[LBM_MSG_MAX_TOPIC_LEN]

Application source ID as a null-terminated string.

unsigned char lbmmon_packet_attributes_t_stct::mContextInstance[LBM_CONTEXT_INSTANCE_BLOCK_SZ]

Context Instance of the object being monitored.

lbm_uint32_t lbmmon_packet_attributes_t_stct::mDomainID

Domain ID of the object being monitored.

uint64_t lbmmon_packet_attributes_t_stct::mFlags

For internal use only.

lbm_ushort_t lbmmon_packet_attributes_t_stct::mModuleID

Module ID of the sent packet.

lbm_uint64_t lbmmon_packet_attributes_t_stct::mObjectID

Object ID of the object being monitored.

lbm_ushort_t lbmmon_packet_attributes_t_stct::mPacketAttributesMagic

"Magic" value must be LBMMON_ATTR_BLOCK_MAGIC.

lbm_uint64_t lbmmon_packet_attributes_t_stct::mProcessID

Process ID of the object being monitored.

lbm_ushort_t lbmmon_packet_attributes_t_stct::mSourceFlag

Source Flag. See LBMMON_ATTR_SOURCE_* for possible values.

time_t lbmmon_packet_attributes_t_stct::mTimestamp

Timestamp of the sent packet.

The documentation for this struct was generated from the following file:

- lbmmon.h