UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_src_event_sequence_number_info_t_stct Struct Reference

Structure that holds sequence number information for a message sent by a source. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap set of flags reserved for future use. Currently set to 0.
lbm_uint_t | first_sequence_number
| First sequence number for the message set.
lbm_uint_t | last_sequence_number
| Last sequence number for the message set.
void * | msg_clientd
| The clientd pointer passed in for the message.

## Detailed Description

Structure that holds sequence number information for a message sent by a source.

This structure signals to the source the assignment of sequence numbers to an outgoing message. It indicates the starting and ending sequence numbers assigned to the message. Delivered as a source event LBM_SRC_EVENT_SEQUENCE_NUMBER_INFO via callbacks lbm_src_cb_proc and lbm_ssrc_cb_proc, but only when enabled by sending the message using the lbm_src_send_ex() function and setting the LBM_SRC_SEND_EX_FLAG_SEQUENCE_NUMBER_INFO flag or LBM_SRC_SEND_EX_FLAG_SEQUENCE_NUMBER_INFO_FRAGONLY flag.

See lbm_src_event_sequence_number_info_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h