UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
tnwg_portal_peer_dstat_record_t_stct Struct Reference

Structure containing sending and receiving statistics for a peer portal. More...

`#include <tnwgdmonmsgs.h>`

## Data Fields
tnwg_dstat_peer_receive_stats_t | receive_stats
| Receiving statistics.
tnwg_dstat_peer_send_stats_t | send_stats
| Sending statistics.
uint32_t | ingress_cost
| Cost.
uint32_t | local_interest_topics
| Number of local interest topics.
uint32_t | local_interest_pcre_patterns
| NOT USED. Set to zero.
uint32_t | local_interest_regex_patterns
| NOT USED. Set to zero.
uint32_t | remote_interest_topics
| NOT USED. Set to zero.
uint32_t | remote_interest_pcre_patterns
| Number of remote interest pcre patterns.
uint32_t | remote_interest_regex_patterns
| Number of remote interest regex patterns.
uint32_t | proxy_receivers
| Number of proxy receivers.
uint32_t | receiver_topics
| Number of receiver topics.
uint32_t | receiver_pcre_patterns
| Number of receiver pcre patterns.
uint32_t | receiver_regex_patterns
| Number of receiver regex patterns.
uint32_t | proxy_sources
| Number of proxy sources.
uint32_t | udp_peer
| True when UDP Peer is configured.
tnwg_dstat_peer_udp_receive_stats_t | udp_receive_stats
| UDP Receive statistics.
tnwg_dstat_peer_udp_send_stats_t | udp_send_stats
| UDP Send statistics.

## Detailed Description

Structure containing sending and receiving statistics for a peer portal.

Used by tnwg_portalstats_dstat_record_t. Except where indicated, all fields of type `lbm_uintXX_t` should be byte-swapped if `hdr.magic` is equal to LBM_TNWG_DAEMON_ANTIMAGIC.

Note that fields remote_interest_topics, remote_interest_pcre_patterns, and remote_interest_regex_patterns are not used by peer portals, and are set to zero.

The documentation for this struct was generated from the following file:

- tnwgdmonmsgs.h